**Terms and conditions for assembly quotes.**

**1. Workmanship standard: ANSI/J-STD-001class II & IPC-A-610 E class II or customer's spec if specified in this quote.**

**2. Standard warranty: 6 Months for workmanship defect not including materials' defect.**

**3. Please provide electronic copies of BOM, Gerber files & CAD data for stencil and programming or extra charge may apply.**

**4. There may be additional cost and lead time if data cannot be provided on item #3.**

**5. For Consignment Parts: SMT components must be supplied to include 10% attrition and min 12” leader tape. IC’s, Relays…. Exact qty needed can be supplied**

**6. For Turn-Key Orders: Customer is responsible for MOQ's (Minimum order quantity), excess materials, obsolete parts, NCNR's**

**(Non-cancel/Non-returnable) and all restocking fees.**

**7. Phase 3 reserves the right to invoice for all raw materials and / or finished product(s) if not shipped within 30 days Unless prior agreement is made.**

**8. Functional Test's software & hardware to be provided by customer and the yield rate to be discussed with customer**

**9. Test charges are normally not included unless specified above.**

**9. The quoted Turn Time starts after material completion, after 24 hr kit audit, stencil preparation and PNP programming.**

**10. The above quote is good for 30 days unless otherwise noted.**

**11. Material quotes are subject to component availability and component lead times at the time the quote is issued.**

**11. Please state on your purchase order if this is a ITAR, medical or medical related device.**